

|  |
| --- |
| **14" PROFESSIONAL COLOR MONITOR**     High Reliability 1 way AUDIO    Best Performance Fully Digital Control    High resolution On Screen Display    S-VHS Input NTSC / PAL Auto    High-Impedance Input Universal AC Power |

|  |  |  |
| --- | --- | --- |
|  |  | |
|  | | :: SPECIFICATION |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | |  |  |  | | --- | --- | --- | | **ITEM** | | **SPECIFICATION** | | **PRODUCT** | | **14" HIGH RESOLUTION PROFESSIONAL           COLOR MONITOR** | | **RESOLUTION** | | **OVER THAN 460 TV-LINES** | | **VIDEO** | | **NTSC / PAL AUTO** | | **AUDIO** | | **1 way AUDIO** | | **AC POWER** | | **UNIVERSAL AC POWER (90~240VOLT, 50/60Hz)** | | **FEATURE** | | **SVHS VIDEO-IN          HIGH-IMPEDANCE VIDEO IN          DIGITAL CONTROL          ON SCREEN DISPLAY** | | **CONNECTORS** | **VIDEO** | **CAMERA IN --- 1 pc OF BNC CONNECTOR          SLAVE IN --- 1 pc OF SVHS CONNECTOR          SVHS IN --- 1 pc OF SVHS CONNECTOR          VCR IN --- 1pc OF RCA CONNECTOR          VCR OUT --- 1pc OF RCA CONNECTOR** | | **AUDIO** | **CAMERA IN --- 1 pc OF RCA CONNECTOR          SLAVE IN --- 1 pc OF RCA CONNECTOR          VCR IN --- 1 pc OF RCA CONNECTOR          VCR OUT --- 1 pc OF RCA CONNECTOR** | | **CABINET** | | **PLASTIC FRONT MASK AND METAL BODY** | | **DIMENSION** | | **W365   D390   H338mm** | | **STUFFING** | | **325 set / 20ft,   675 set / 40ft** | | **\* Specification are subject to change without notice** | | | |

|  |  |
| --- | --- |
|  | :: Front & Back Control |

|  |  |
| --- | --- |
|  |  |